Laser-cavity locking utilizing beam ellipticity: accessing the 10<sup>7</sup> instability scale relative to cavity linewidth